
; ----------------------------------------------------------------------

.Patch Names


[Line 6 POD Patches]
0=Manual Mode
1=1A: Big Rectifier
2=1B: Black Panel
3=1C: POD Clean
4=1D: POD Drive
5=2A: Small Twead
6=2B: Dumble (Rotary)
7=2C: POD Clean Auto Swell
8=2D: Bassman (Slapback Echo)
9=3A: POD Clean (Comp)
10=3B: POD Crunch (Reverb)
11=3C: POD Drive (Delay)
12=3D: POD Layer (Lt. Chorus & Dly)
13=4A: Small Tweed (Reverb) (1952 Fender Deluxe)
14=4B: Tweed Blues (1959 Fender Bassman)
15=4C: Black Panel (1964 Fender Deluxe)
16=4D: Modern Class A (Matchless Chieftain)
17=5A: Brit Class A (1960 VOX ACI 5)
18=5B: Brit Blues (1965 Marshall JTM-45)
19=5C: Brit Classic (1968 Marshall "Plexi")
20=5D: Brit Hi Gain (1986 Marshall JCM 800)
21=6A: Rectified (Mesa Boogie Dual Rectifier Tremo-O-Verb)
22=6B: Modern Hi Gain (Soldano X88 Preamp)
23=6C: Fuzz Box (Arbitor Fuzzface)
24=6D: Tube Preamp (direct recording of non-guitar instruments)
25=7A: Jazz Clean (Chorus) (Roland JC120)
26=7B: Small Twead #2 (1961 Fender Champ)
27=7C: Black Panel #2 (1965 Fender Twin)
28=7D: Brit Class A #2 (1960 VOX AC30)
29=8A: Brit Class A #3 (Echo) (1966 VOX AC30 Top Boost)
30=8B: Boutique #1 (Dumble Overdrive Special Clean)
31=8C: Boutique #2 (Lt. slapback) (Dumble Overdrive Special Drive)
32=8D: Boytique #3 (Budda Twinmaster)
33=9A: California Crunch #1 (Mesa Boogie Mark IIC+ Clean
34=9B: California Crunch #2 (Mesa Boogie Mark IIC+ Crunch)
35=9C: Rectified #2 (Mesa Boogie Dual Rectifier Head)
36=9D: Modern Hi Gain #2 (Soldano SLO Super Lead Overdrive)
37=Tuner

; ----------------------------------------------------------------------

.Note Names


; ----------------------------------------------------------------------

.Controller Names


[Line 6 POD Controllers]
1=1: Effect Tweak
4=4: Wah Pedal
7=7: Volume Pedal
12=12: Amp Model (0=Tube preamp; 1-27=Other Amp Models)
13=13: Drive
14=14: Bass
15=15: Mid
16=16: Treble
17=17: Channel Volume
18=18: Reverb Level
19=19: Effect Select Knob (0=Bypass; 1-15=Other Effects)
20=20: Drive 2
21=21: Presence
22=22: Noise Gate On/Off (0-63=OFF; 64-127=ON)
23=23: Gate Threshold
24=24: Gate Decay
25=25: Distortion On/Off (0-63=OFF; 64-127=ON)
26=26: Drive/Boost (0-63=OFF; 64-127=ON)
27=27: EQ (presence Bump) (0-63=OFF; 64-127=ON)
28=28: Delay (0-63=OFF; 64-127=ON)
29=29: Delay Type (0-63=MONO; 64-127=STEREO)
30=30: Delay Time 1
31=31: Delay Time 2 (stereo only)
32=32: Delay Regeneration 1
33=33: Delay Regeneration 2 (stereo only)
34=34: Delay Level 1
35=35: Delay Level 2 (stereo only)
36=36: Reverb (0-63=OFF; 64-127=ON)
37=37: Reverb Type (0-63=SPRING; 64-127=HALL)
38=38: Reverb Decay
39=39: Reverb Tone
40=40: Reverb Diffusion
41=41: Reverb Density
42=42: Compression Ratio (0-21=OFF; 22-44=1.4:1; 45-67=2:1; 68-90=3:1; 91-113=6:1; 114-127=infinity:1)
43=43: Wah Wah Pedal On/Off (0-63=OFF; 64-127=ON)
44=44: Wah Bottom Frequency
45=45: Wah Top Frequency
46=46: Volume Pedal Minimum
47=47: Volume Pedal Location (0-63= Before Tube; 64-127=After Tube)
48=48: Volume Swell On/Off (0-63=OFF; 64-127=ON)
49=49: Volume Swell Ramp Time
50=50: Chorus/Rotary/Tremolo On/Off (0-63=OFF; 64-127=ON)
51=51: Chorus/Flange Speed
52=52: Chorus/Flange Depth
53=53: Chorus/Flange Regen (0-63=Negative; 64-127=Positive)
54=54: Chorus PreDelay
55=55: Rotary Speed
56=56: Rotary Max Speed
57=57: Rotary Min Speed
58=58: Tremolo Speed
59=59: Tremolo Depth
62=62: Double-precision control for Delay Time 1
63=63: Double-precision control for Delay Time 2
64=64: Tap Tempo
71=71: Cabinet Type
72=72: A.I.R. Ambience Level
73=73: Bright Switch (0-63=OFF; 64-127=ON)

; ----------------------------------------------------------------------

.Instrument Definitions


[Line 6 POD]
Control=Line 6 POD Controllers
Patch[*]=Line 6 POD Patches
